
Record web by Jmeter behind Bosch Proxy


1. Access to the folder where you store Jmeter -> Run CMD




1. Run Jmeter with the command line

Jmeter –H rb-proxy-de.bosch.com –P 8080 –N localhost




1. 




Then Click OK


1. Open the browser that you want to record, in this case I using IE

Open IE -> Click Setting -> Choose Internet options



Click Connections Tab -> Choose Lan settings






* Click OK


1. Add Jmeter Certificate to web Browser

Click on Content Tab -> Choose Certificates




Choose Trusted Root Certification Authorities Tab -> Click Import

Click Next



Click Browse -> choose ApacheJmeter….crt -> it was stored in Jmeter/bin Folder -> Click Open



Click Next -> Next -> Finish.

Click Close -> OK.

You are already to record. Start your work and jmeter will automate recording your work. When you finish it, go back to Jmeter and Click Stop